SWPPP Template – Instructions
UDOT has adopted and modified this Storm Water Pollution Prevention Plan (SWPPP) template developed by the DWQ for construction sites permitted under the Construction General Storm Water Permit (CGP). The template gives you a framework to ensure that your SWPPP addresses the necessary elements required by the permit. It may be helpful to use this template with EPA’s guidance on Developing Your Storm Water Pollution Prevention Plan (EPA SWPPP Guide).
Both are available on DWQ’s construction storm water website at https://deq.utah.gov/water-quality/general-construction-storm-water-updes-permits
This template covers most of the SWPPP elements that the Utah CGP requires, however, you are encouraged to customize this template to reflect unique conditions at the site or address a requirement not covered in the provided sections.
Using the SWPPP Template
Each section of this template includes instructions and space for project information. You should read the instructions for each section before you complete that section. If you require additional clarification, the instructions often reference a permit section where you can find the exact wording for the requirement as well as other resources that may be useful. For a cleaner document you may want to delete instructions when finished. Some sections may require only a brief description or not apply at all to your project, while others may require several pages of explanation.
Tips for completing the SWPPP template


· If there is more than one key player affecting stormwater for your project, consider coordinating development of your SWPPP with the other key players.
· Make sure you inform subcontractors about limitations or special requirements if their work intersects with SWPPP requirements. You might write a section of your SWPPP specifically for a subcontractor and deliver that section to the subcontractor before their work commences.
· Modify this SWPPP template so that it addresses the requirements in your construction general permit and meets the needs of your project. Be sure to include important aspects of the SWPPP that go beyond the boundaries of the project.
· EPA’s guidance on Developing Your Storm Water Pollution Prevention Plan (SWPPP Guide) can be accessed here: https://www3.epa.gov/npdes/pubs/sw_swppp_guide.pdf

Stormwater Pollution Prevention Plan
UDOT Region: 
Project Name: 
Project Number:
Project PIN:
Project Location:
Project Coordinates:

SWPPP Preparation Date:
  /  / 
UPDES Permit Tracking Number*:
UTR	

*This is the unique number assigned to your project after you have applied for coverage under the Utah Pollutant Discharge Elimination System (UPDES) construction general permit. If this template is filled out first, you can leave the tracking number blank until after you have applied for coverage.
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SECTION 1: CONTACT INFORMATION/ RESPONSIBLE PARTIES

	Instructions (CGP 6.1 and 7.3.1):
― Identify the staff members that are part of the project’s stormwater team. Include documentation showing training the members of the team who will conduct inspections have received. The stormwater team is comprised of individuals who are responsible for the development of the SWPPP, any later modifications to it, installing and maintaining stormwater controls, conducting site inspections, and making corrective actions where required. 
― Each member of the stormwater team must have ready access to either an electronic or paper copy of the most current CGP and the SWPPP.
― A SWPPP writer for a site greater than 5 acres, with a perennial surface water within 50 feet of the project, or with a steep slope (70% or 35 degrees or more) must hold a certification to demonstrate that they are a “qualified person” per CGP Part 7.2. A certification page is located in Section 11.
―  The following personnel, at a minimum, must receive training on their responsibilities (CGP Part 6.1/6.2):
· Personnel who are responsible for the design, installation, maintenance, and/or repair of stormwater controls (including pollution prevention measures);
· Personnel responsible for the application and storage of treatment chemicals;
· Personnel who are responsible for conducting inspections (must hold a certification) as required in Part 4.1
· Personnel who are responsible for taking corrective actions as required in Part 5.
―  A sample training log is provided in Appendix F. Certifications can also be recorded in this appendix.
―  For more on training, see EPA SWPPP Guide, Chapter 8.




1. Stormwater Team
	General Contractor:
	General Contractor’s ECS:

	Company Name:
Address:
City, State, Zip Code:
Project Foreman’s Name:
Cellphone Number:
Email:
	Company Name:
Address:
City, State, Zip Code:
Project ECS’ Name:
Cellphone Number:
Email:

	UDOT Resident Engineer:
	UDOT ECS:

	Company Name:
Address:
City, State, Zip Code:
Resident Engineer Name:
Cellphone Number:
  Email:
	Company Name:
Address:
City, State, Zip Code:
UDOT ECS’ Name:
Cellphone Number:
Email:

	Subcontractor Responsible for Installing Erosion Control Measures (if not Contractor):
	Other Stormwater Contacts (if applicable):

	Company Name:
Address:
City, State, Zip Code:
Subcontractor Name:
Cellphone Number:
  Email:
	Company Name:
Address:
City, State, Zip Code:
Name:
Cellphone Number:
  Email:


    SECTION 2: NATURE OF CONSTRUCTION ACTIVITIES
1. Construction Site Estimates

	Instructions (CGP 7.3.2.b-c):
― Estimate the area to be disturbed by excavation, grading, or other construction activities, including dedicated off-site borrow and fill areas.



	The following are estimates for the construction site.
	

	Total project area:
	acres

	Construction site area to be disturbed :
	acres




0. Construction Activity Descriptions

	Instructions (CGP 7.3.2.a, d & g):
―  Briefly describe the nature of the construction activity and approximate time frames.
―  For more information see CGP Part 7.3.2 and EPA SWPPP Guide, Chapter 3.A.



	Describe the general scope of the work for the project, major phases of construction, etc.:
	INSERT TEXT HERE

	Describe any on-site and off-site construction support activity areas and staging areas:
	INSERT TEXT HERE


















0. Phase/Sequence of Construction Activity

	Instructions (CGP 7.3.2.e):
― List the intended construction sequencing and timing of major activities, including phasing, grading, and stabilization activities. Be mindful of opportunities for timing grading and stabilization so that all or a majority of the soil disturbance occurs during a time of year with less erosion potential (i.e., during the dry or less windy season).
― For more information, see EPA SWPPP Guide, Chapter 4, ESC Principle 2. It might be useful to develop a separate, detailed site map for each phase of construction.



	Construction Activity 
	Estimated Start 
Date
	Estimated End 
Date

	Project Start (after NOI) and End
	
	

	Clearing and Grubbing
	
	

	Excavation (earthwork)
	
	

	Seasonal Shutdown (if applicable)
	
	

	Final Grading
	
	

	Temporary Stabilization
	
	

	Removal of Stormwater Control Measures and Cessation of Pollutant Generating Activity
	
	

	Final Stabilization (may extend beyond project close out)
	
	


[Insert or delete rows as necessary.]

    SECTION 3: WATER QUALITY
1. Discharge Information

	Instructions (CGP 1.4):
― A Municipal Separate Storm Sewer System (MS4) is a stormwater conveyance system owned and operated by a state, city, town, county, district, association, or other public body. If you discharge to one of these systems mark “yes” and identify which MS4.You must submit your SWPPP to this MS4 for review. A list of MS4s that are currently designed under a Utah municipal stormwater permit can be found here: https://deq.utah.gov/water-quality/municipal-separate-storm-sewer-system-ms4s-permits-updes-permits 



	Does your project/site discharge stormwater into a Municipal Separate Storm Sewer System (MS4)?	Yes	No

	List the MS4 that receives the discharge from the construction project: INSERT TEXT HERE




0. Receiving Waters

	Instructions (CGP 1.1.6 and 3.1):
― In the below table, list the name of the first waters of the state that would receive discharges from your site. Multiple rows are provided in case your site discharges in multiple locations which flow to different waters of the state. For discharges that enter a storm sewer system prior to discharge, the first waterbody to which you discharge is the waterbody that receives the stormwater discharge from the storm sewer system. You may need to contact the storm sewer system owner to find out where it discharges to.
― See https://deq.utah.gov/water-quality/water-quality-assessment-map for impairment or quality information. Use this to identify the status in column 2 of the table below. Select the waterbody you wish to look up and find the results from the 20XX Assessment on the left hand side.
― For more information on TMDLs and impaired waters visit https://deq.utah.gov/water-quality/watershed-protection/state-and-federally-approved-total-maximum-daily-load-studies or https://www.epa.gov/tmdl/impaired-waters-and-stormwater. 
― If any of the waters of the state you listed are impaired, provide specific information about pollutants causing the impairment in column 3 of the table below. Your SWPPP should specifically include measures to prevent the discharge of these pollutants.
― If any of the waters of the state you listed are identified as a Category 1 or 2 water (a Category 1 water is only found within Forest Service boundaries) provide the category in column 3 of the table below.
―  For more information, see CGP Part 3.1 and 3.2 and EPA SWPPP Guide, Chapter 3.B.





Names of Receiving Waters
	Name of Receiving Water (first waters of the state that receives stormwater or where storm system discharges to)
	Is the water impaired or high quality?
	If high quality: Is it Category 1 or 2?
If impaired: List pollutants that the waterbody is impaired for

	1.
	Not high quality/impaired Impaired, has approved TMDL Impaired, no TMDL
High quality
	

	2.
	Not high quality/impaired Impaired, has approved TMDL Impaired, no TMDL
High quality
	


[Insert or delete rows as necessary.]


0. Impaired Waters

	Instructions (CGP 3.2):
― If you discharge to an impaired water as listed in the above table, provide information on additional efforts that will be taken to control the release of impairment causing pollutants. This is especially important for projects discharging to a surface water with an EPA approved TMDL for sediment or nutrients and an extra effort must be provided to prevent sediment from leaving the site.



Description of additional precautions taken if discharging to impaired waters of the state. State if no impairment causing pollutants are on site:
INSERT TEXT HERE


0. High Water Quality

	Instructions (CGP 3.2):
― If you discharge to a high-quality water as listed in the table above, provide information on additional efforts that will be taken to control the release of pollutants. Per CGP Part 1.1.6 you can discharge to a Category 1 water if your discharge is temporary and limited and where best management practices will be employed to minimize pollution effects. Discharge to Category 2 waters is allowed only if the discharge will not lower the water quality of the water body.



Description of additional precautions taken to minimize pollution effects if you are discharging to a high-quality surface water:
INSERT TEXT HERE

SECTION 4: POLLUTION PREVENTION STANDARDS
1. Potential Sources of Pollution

	Instructions (CGP 7.3.2.f):
― Identify and list all potential sources of sediment, which may reasonably be expected to affect the quality of stormwater discharges from the construction site.
― Identify and describe all potential sources of pollution or pollutant-generating activity (e.g., paving operations; concrete, paint, and stucco washout and waste disposal; solid waste storage and disposal), other than sediment, which could be exposed to rainfall or snowmelt, and may reasonably be expected to discharge from the construction site.
      ― For more information, see EPA SWPPP Guide, Chapter 3.A.



	
Pollutant-Generating Activity
	Pollutants or Pollutant Constituents
(that could be discharged if exposed to stormwater)
	Location on Site
(or reference SWPPP site map where this is shown)

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	

	
	
	


[Include additional rows as necessary.]

0. Non-Stormwater Discharges

	Instructions (CGP 7.3.4):
― Identify all allowable sources of non-stormwater discharges and how they will be controlled. A list of allowable non-stormwater discharges is found in the CGP Part 1.2.2.
―  For more information, see EPA SWPPP Guide, Chapter 3.A.



Check allowable non-stormwater discharges that are present and describe the measures used to reduce them or prevent them from contributing pollutants to discharges:

	Authorized Non-Stormwater Discharges
	Present
	Comments/Controls

	Discharges from emergency fire-fighting
activities
	Y
	N
	

	Fire hydrant flushing
	Y
	N
	

	Properly managed landscape irrigation (excludes fertilizer injector systems)
	
Y
	
N
	

	Properly managed vehicle and
equipment wash water with no soaps, solvents, or detergents
	
Y
	
N
	

	Water used to control dust
	Y
	N
	

	Drinking water, including uncontaminated
water line flushing
	Y
	N
	

	External building washdown with no soaps,
solvents, detergents, or hazardous substances
	Y
	N
	

	Pavement wash waters with no detergents or toxic or hazardous materials. Must have a sediment basin, sediment trap, of similarly
effective control prior to discharge
	
Y
	
N
	

	Uncontaminated air conditioning or
compressor condensate
	Y
	N
	

	Uncontaminated, non-turbid
discharges of groundwater (from natural sources) or spring water
	
Y
	
N
	

	Uncontaminated foundation or footing drains
	
Y
	
N
	





0. Dewatering Practices

	Instructions (CGP 1.2.4 and 2.3.7):
If you will be discharging stormwater that is removed from excavations, trenches, foundations, vaults, or other similar points of accumulation, it must be permitted by UPDES permit UTG070000 (Construction Dewatering and Hydrostatic Testing Permit) unless it can be managed onsite through percolation or evaporation. The permit can be found at https://deq.utah.gov/water-quality/general-construction-storm-water-updes-permits in the bottom table. Call DWQ at 801-536-4300 for more information.
―  Include schedule and general locations of dewatering. Dewatering locations must be on the site map.



[image: ] Check box if section not applicable to this site (Note: If not applicable skip to next section)

Describe the general scope of dewatering practices for the project and any BMPs used to manage the dewatering practices:
INSERT TEXT HERE
































0. Natural Buffers or Equivalent Sediment Controls

	Instructions (CGP Part 7.3.5.b (1), 2.2.1, and Appendix A):
This section only applies if waters of the state are located within 50 feet of your construction activities. If this is the case, review CGP Part 2.2.1 and Appendix A of the CGP for information on how to comply with the buffer requirements.
― Describe the compliance alternative that was chosen to meet the buffer requirements and include any required documentation supporting the alternative selected. The compliance alternative selected must be maintained throughout the duration of permit coverage. However, if you select a different compliance alternative during your period of permit coverage, you must modify your SWPPP to reflect this change.
― If you qualify for one of the exceptions in CGP Part A.2.2, include documentation related to your qualification for such exceptions.
― Review Appendix A of the CGP for step-by-step instructions and examples on how to comply with the different buffer alternatives.



Buffer Compliance Alternatives
Are there any waters of the state within 50 feet of your project’s earth disturbances? [image: ] YES	[image: ] NO
(Note: If “no”, no further documentation is required. Delete the rest of Section 4.3 below this point.)

List the water body: INSERT TEXT HERE

Check the compliance alternative that you have chosen:
[image: ] I will provide and maintain a 50-foot undisturbed natural buffer around waters of the state.

[image: ] It is infeasible to provide and maintain a full 50-foot undisturbed natural buffer. I will provide and implement erosion and sediment controls to achieve the required sediment load reduction for my conditions.
· Reason that a 50’ buffer could not be maintained: INSERT TEXT HERE
· Width of buffer that will be retained: INSERT TEXT HERE
· Additional controls used to achieve equivalent sediment load reduction of a 50’ buffer: INSERT TEXT HERE
· Description of the calculations and assumptions used to determine sediment load reductions: INSERT TEXT HERE


[image: ] I qualify for one of the exceptions in Part A.2.2. (If you have checked this box, provide information on the applicable buffer exception that applies, below.)
[image: ] There is no discharge of stormwater through the area between the disturbed portions of the site and waters of the state that is located within 50 feet.

[image: ] No natural buffer exists due to preexisting development disturbances that occurred prior to the initiation of planning for this project.

[image: ] For a linear project, site constraints (e.g., limited right-of-way) make it infeasible for me to meet any of the compliance alternatives.
· Reason it is infeasible: INSERT TEXT HERE
· Buffer width retained or supplemental controls used: INSERT TEXT HERE

[image: ] Buffer disturbances are authorized under a CWA Section 404 permit.
· Describe earth disturbances in buffer area: INSERT TEXT HERE
(Note: This exception does not apply to portions upland of the Section 404 permitted work.)

[image: ] Buffer disturbances will occur for the construction of a water-dependent structure or water access area (e.g., pier, boat ramp, and trail).
· Describe earth disturbances in buffer area: INSERT TEXT HERE

SECTION 5: EROSION AND SEDIMENT CONTROLS – BMPS
1. List of Erosion and Sediment BMPs on Site

	Instructions (CGP Part 2.2 and 7.3.5):
― Identify best management practices (BMPs) that will be implemented on site to control erosion and sediment transport from stormwater.
―  BMPs are listed as examples; you may use BMPs not listed.
― Temporary erosion and sediment controls will be installed and maintained according to UDOT Standards and Specifications https://connect.udot.utah.gov/business/standards/ 
― Perimeter control maintenance must include removal of sediment before it has accumulated to one-half the above-ground height of the control.
―  For more information, see EPA SWPPP Guide, Chapter 4.
― BMP guidance may be found in your MS4’s or other local jurisdiction’s design manual, guidance manuals listed in Appendix D of the EPA SWPPP Guide, or EPA’s National Menu of BMPs https://www.epa.gov/npdes/national-menu-best-management-practices-bmps-stormwater#constr 



	Check 
All 
That 
Apply
	Temporary Control 
Description
	UDOT Standards
	When Will Control 
Measure be 
Implemented? 

	
	
	Drawing 
	Specification 
	

	
	Fiber Roll Check Dam 
	EN 1 
	01571
	

	
	Stone Check Dam 
	EN 1 
	01571
	

	
	Silt Fence 
	EN 2 
	01571
	

	
	Temporary Berm 
	EN 3 
	01571
	

	
	Temporary Slope Drain 
	EN 3 
	01571
	

	
	Fiber Roll Drop Inlet 
Barrier 
	EN 4 
	01571
	

	
	Silt Fence Drop Inlet 
Barrier 
	EN 4 
	01571
	

	
	Pipe Inlet Barrier 
	EN 5 
	01571
	

	
	Gutter Inlet Barrier 
	
	01571
	

	
	Sediment Trap 
	EN 6 
	01571
	

	
	Stabilized Construction Entrance 
	EN 6 
	01571
	

	
	Straw Bale Barrier 
	EN 7 
	01571
	

	
	Hydraulic Erosion Control Product (Type 1, 2, or 3) 
	
	02911
	

	
	Erosion Control Blanket 
	
	02376
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	






0. List of Post Construction (Permanent) Controls

	Instructions (CGP Part 2.2 and 7.3.5):
― Identify best management practices (BMPs) that will be installed onsite to reduce the discharge of pollutants to receiving waters. 
― Post construction controls include Low Impact Development (LID) measures and traditional measures such as detention basins, flow restriction devices, and floating debris traps. LID measures are different as they manage stormwater as close to the source as possible rather than conveying stormwater elsewhere for treatment.
―  BMPs are listed as examples; you may use BMPs not listed.
― Post construction stormwater control measures will be installed and maintained according to project detail 
       drawings and specifications. 
― BMP guidance may be found in your MS4’s or other local jurisdiction’s design manual, guidance manuals listed in Appendix D of the EPA SWPPP Guide, or EPA’s National Menu of BMPs https://www.epa.gov/npdes/national-menu-best-management-practices-bmps-stormwater-post-construction. 



	Check 
All 
That 
Apply
	Post Construction Control
Description
	Project Details
	Targeted Pollutants 

	
	
	Drawing 
	Specification
	

	
	Preserve Existing Vegetation*
	
	
	

	
	Sheet Flow Off Pavement*
	
	
	

	
	Vegetated Landscaping*
	
	
	

	
	Erosion Control Blanket 
	
	02376
	

	
	Flexible Channel Liner 
	
	02376
	

	
	Turf Reinforcement Mat*
	
	02376
	

	
	Hydraulic Erosion Control 
Products (Type 1, 2, or 3) 
	
	02911
	

	
	Broadcast or Drill Seed 
	
	02922
	

	
	Rock Mulch Landscaping*
	
	
	

	
	Rock Lined or Vegetated Swale*
	
	
	

	
	Riprap Lined Ditch
	
	
	

	
	Detention Basin
	
	
	

	
	Retention Basin
	
	
	

	
	Wet Pond
	
	
	

	
	Constructed Wetland 
	
	
	

	
	Permeable Friction Course*
	
	
	

	
	Shoulder Dressing*
	
	
	

	
	Catch Basin with Hooded Outlet Cover
	
	
	

	
	Catch Basin with Lowered Invert
	
	
	

	
	Riprap / Stilling Basin at Culvert Outlet
	
	
	

	
	Energy Dissipator Structure
	
	
	


                *Post Construction Control is LID. 



0. Linear Site Perimeter Control Exemption

	Instructions (CGP 7.3.5.b (2)):
― For areas where perimeter controls are not feasible on a linear construction site, include a description of why it is not feasible and other practices that will be implemented to minimize discharges of pollutants from the site.



[image: ] Check box if section not applicable to this site (Note: If not applicable skip to next section)
If the site is linear and perimeter controls are not feasible, describe other practices in use:
INSERT TEXT HERE



0. Final Stabilization

	Instructions (CGP 7.3.5.b (6) and 2.2.14.b):
― Describe procedures for final stabilization. If the final cover is vegetation, you must establish uniform perennial vegetation that provides 70% or more of the vegetative cover that existed prior to earth-disturbing activities. Exception: Arid, semi-arid, and drought-stricken areas are required to be seeded/planted so that the before mentioned vegetative requirement is expected to be met within 3 years. Establishment of vegetation is not required; however additional erosion controls may be needed.
―  You can amend or add to this section as areas of your project are finally stabilized.
―  Update your site plans to indicate areas that have achieved final stabilization.



Description of final stabilization practices and schedule:

	Type of stabilization (vegetation/landscaped, graveled, paved, etc.)
	Location
	Implementation Schedule

	
	
	

	
	
	

	
	
	

	
	
	





SECTION 6: BMPS - POLLUTION PREVENTION/OPERATIONAL CONTROLS
1. Spill Prevention and Response

	Instructions (CGP Part 7.3.5.b (7) and 2.3.6):
― Describe the spill prevention and control plan. Include ways to reduce the chance of spills, stop the source of spills, contain and clean up spills, dispose of materials contaminated by spills, and train personnel responsible for spill prevention and control.
― Some projects/sites may be required to develop a Spill Prevention Control and Countermeasure (SPCC) plan under a separate regulatory program (40 CFR 112). If you are required to develop an SPCC plan, or you already have one, you should include references to the relevant requirements from your plan.
― The plan must include the materials and method of containment, procedures for cleanup and disposal, and must report the minimum spill controls below.
― For more information on UDOT’s general spill plan, see Appendix C of the SWPPP.
―  For more information, see EPA SWPPP Guide, Chapter 5, P2 Principle 6.



Describe spill procedures and materials available for expeditious containment, clean-up and disposal of spills:
INSERT TEXT HERE OR REFERENCE DOCUMENT

Identify the employee responsible for detection and response of spills and leaks:
INSERT TEXT HERE

Any discharges in 24 hours equal to or in excess of the reportable quantities listed in 40 CFR 117, 40 CFR 110, and 40 CFR 302 will be reported to the National Response Center and the Division of Water Quality (DWQ) as soon as practical after knowledge of the spill is known to the permittees. The permittee shall submit within 7 calendar days of knowledge of the release a written description of: the release (including the type and estimate of the amount of material released), the date that such release occurred, the circumstances leading to the release, and measures taken and/or planned to be taken to the Division of Water Quality (DWQ), 288 North 1460 West, P.O. Box 144870, Salt Lake City, Utah 84114-4870. The Stormwater Pollution Prevention Plan must be modified within 14 calendar days of knowledge of the release to provide a description of the release, the circumstances leading to the release, and the date of the release. In addition, the plan must be reviewed to identify measures to prevent the recurrence of such releases and to respond to such releases, and the plan must be modified where appropriate.

	Agency
	Phone Number

	National Response Center
	(800) 424-8802

	Division of Water Quality (DWQ) 24-Hr Reporting
	(801)-231-1769
(801) 536-4123

	Utah Department of Health Emergency Response
	(801) 580-6681



	Material
	Media Released To
	Reportable Quantity

	Engine oil, fuel, hydraulic & brake fluid
	Land
	25 gallons

	Paints, solvents, thinners
	Land
	100 lbs (13 gallons)

	Engine oil, fuel, hydraulic & brake fluid
	Water
	Visible Sheen

	Antifreeze, battery acid, gasoline, engine degreasers
	Air, Land, Water
	100 lbs (13 gallons)

	Refrigerant
	Air
	1 lb


0. Pollution Prevention Controls

	Instructions (CGP Part 2.3 and 7.3.5):
― Describe the key good housekeeping and pollution prevention BMPs that will be implemented to control pollutants in stormwater (CGP Part 2.3).
― Use the CGP requirements and the pollutant generating activities identified in SWPPP section 4.1. which were not addressed with the erosion and sediment BMPs to determine where BMPs are necessary.
―  BMPs are listed as examples, you may use BMPs not listed.
―  For more information, see EPA SWPPP Guide, Chapter 5.
― For more information or ideas on BMPs, see EPA’s National Menu of BMPs https://www.epa.gov/npdes/national-menu-best-management-practices-bmps-stormwater#constr 



	Check 
All 
That 
Apply
	Temporary Control 
Description
	UDOT Standards
	When Will Control 
Measure be 
Implemented?

	
	
	Drawing 
	Specification 
	

	
	Concrete Washout 
	
	01355
	

	
	Portable Toilet
	
	
	

	
	Secondary Containment
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	





SECTION 7: SPECIAL CONDITIONS

	Instructions:
The conditions listed below require additional details or actions added to your SWPPP. If they do not apply you may delete them from this SWPPP.




1. Emergency Related Projects

	Instructions (CGP 1.4.1):
― For emergency activities that require immediate authorization but last longer than 30 days, a NOI may be submitted within 30 days of starting work.
― To be an emergency related project it must be considered a public emergency, and the cause must be documented along with the description of necessary construction to reestablish affected public services.


        Emergency-Related Project?	[image: ] Yes	[image: ] No
DESCRIBE THE NATURE OF THE PUBLIC EMERGENCY AND WHY IMMEDIATE AUTHORIZATION WAS NECESSARY.


0. UIC Class 5 Injection Wells

	Instructions (CGP 7.3.7):
― If you are using any of the following stormwater controls at your site as they are described below, you must document any contact you have had with DWQ for implementing the requirements for underground injection wells in the Safe Drinking Water Act and DEQ’s implementing regulation at UAC R317-7-2.
―  There may be additional local requirements related to such structures.
―  For the State UIC Contact at DWQ call (801) 536-4300.



	Check box if section not applicable to this site (Note: If not applicable skip to next section)

Class V UIC Wells on site (all must be reported to DWQ for inventory):
Infiltration trenches (if stormwater is directed to any shaft or hole that is deeper than its widest surface dimension or has a subsurface fluid distribution system)

	Commercially manufactured pre-cast or pre-built subsurface detention
vault/infiltration system

	Drywell, seepage pit, or improved sinkhole (if stormwater is directed to any shaft or hole that is deeper than its widest surface dimension or has a subsurface fluid distribution system)

	Description of your Class V Injection Well and any local requirements:





INSERT DESCRIPTION AND ANY DWQ OR LOCAL REQUIREMENTS
Description of any additional BMPs used in conjunction with the UIC well:
INSERT NAME AND DESCRIPTION OF BMP


0. Chemical Treatment

	Instructions (see CGP 2.2.13 and 7.3.5.b (5)):
― UDOT prohibits the use of treatment chemicals on UDOT projects.





SECTION 8: INSPECTIONS & CORRECTIVE ACTIONS
1. Inspections

	Instructions (CGP Part 4.2, 4.3 and 4.4):
― Select an inspection schedule. These are minimum frequencies; you may inspect more frequently. If so, describe what your schedule would be.
―  For more on this topic, see EPA SWPPP Guide, Chapters 6 and 8.



	Minimum Inspection Schedule Requirements:

	Standard Frequency:

	     Contractor ECS: Once every 7 calendar days.

	     UDOT ECS: Once every 14 calendar days

	Increased Frequency (if applicable):

	    [image: ]   Sites discharging to impaired or high-quality waters – Contractor ECS: Once every
            7 calendar days and within 24 hours of the end of a storm event of 0.5 inches or 
            greater.

	Decreased Frequency (if applicable):

	             Frozen conditions with work suspended – must have 3 months of continuous
expected frozen conditions based on historical averages: no inspections 
List months of suspended inspections (also select the inspection schedule followed when not frozen)

	            Frozen conditions with continued activities - must have 3 months of continuous
expected frozen conditions based on historical averages: once per month 
List months of frozen conditions (also select the inspection schedule followed when not frozen)

	Other:

	            Winter suspended work- must have no active construction and all areas of the site
     must be stabilized: inspections every other week the first month and then monthly
List months of suspended activity (also select the inspection schedule followed when active)
· Describe alternative frequency: 
    List alternative schedule, must meet minimum requirements

	Inspection Reports must be filed in UDOT’s approved inspection software





0. Corrective Actions

	Instructions:
― Whenever a stormwater control requires repair or replacement (beyond routine maintenance), a control necessary for permit compliance was never installed or was installed incorrectly, your discharges cause an exceedance of applicable water quality standards, or a prohibitive discharge has occurred, you must log corrective actions taken.
―  Corrective actions must be logged in the UDOT approved inspection software.





0. Delegation of Authority

	Instructions:
― Identify the individual(s) or specifically describe the position where the construction site operator has delegated authority for the purposes of signing inspection reports, SWPPP documents, corrective action logs, or other information for reporting purposes.
―  Each inspection report must be signed in accordance with CGP Part 9.9.2 of the permit.
― If a delegation letter is necessary, see Appendix E of this template and keep a signed copy with this SWPPP.
―  For more on this topic, see EPA SWPPP Guide, Chapter 7.



See the signed delegation of authority forms in Appendix E.

SECTION 9: RECORDKEEPING


1. Recordkeeping

	Instructions (CGP 7.4, 9.8 and 9.18):
― The following is a list of records you must have accessible on site (electronically or paper) for inspectors to review:
·    The signed and certified NOI form or permit application form (Appendix B)
·    The Stormwater Pollution Prevention Plan (SWPPP)
· A copy of the construction general permit
― Copies of the SWPPP and all reports required by the permit must be retained for at least three years from the date that the site is finally stabilized.
―  For more on this subject, see EPA SWPPP Guide, Chapter 6.C.





SECTION 10: Site Maps

	Instructions (CGP 7.3.3):
― Attach site maps. For most projects, a series of site maps is recommended. The first should show the undeveloped site and its current features. An additional map or maps should be created to show the developed site or for more complicated sites show the major phases of development.
These maps should include the following:
―  Boundaries of the property
―  Locations of earth-disturbing activities, including demolition, and note any phasing;
―  Direction(s) of stormwater flow and approximate slopes before and after major grading activities;
―  Type and extent of pre-construction cover (vegetative cover, pavement, etc.);
―  Locations of stockpiles and material storage;
―  Water crossings and all water of the state within one mile downstream of the site’s discharge point;
―  Designated points where vehicles enter onto paved roads;
―  Locations of structures and other impervious surfaces upon completion of construction;
―  On-site and off-site construction support activity areas covered by the permit;
―  Stormwater and authorized non-stormwater discharge locations to inlets or waters of the state;
―  Locations of all potential pollutant-generating activities;
―  Locations of stormwater controls, including natural buffer areas; and
―  Locations where polymers, flocculants, or other treatment chemicals will be used and stored.
―  For more information, see EPA SWPPP Guide, Chapter 3.C.


The SWPPP site map(s) are filed in Appendix A









SECTION 11: CERTIFICATION

	Instructions:
― The SWPPP should be signed and certified by the owner and the general contractor. Attach a copy of the NOI. You can get a copy of the General Storm Water Permit for Construction Activity on the Department of Environmental Quality’s webpage: https://deq.utah.gov/water-quality/general-construction-storm-water-updes-permits 



UDOT Resident Engineer
I certify under the law that this document and all attachments were prepared under my direction or supervision in accordance with a system designed to assure that qualified personnel properly gathered and evaluated the information submitted. Based on my inquiry of the person or persons who manage the system, or those persons directly responsible for gathering the information, the information submitted is, to the best of my knowledge and belief, true, accurate, and complete. I am aware that there are significant penalties for submitting false information, including the possibility of fine and imprisonment for knowing violations.

	Name:
	Title:

	Signature:
	Date:



General Contractor
I certify under the law that this document and all attachments were prepared under my direction or supervision in accordance with a system designed to assure that qualified personnel properly gathered and evaluated the information submitted. Based on my inquiry of the person or persons who manage the system, or those persons directly responsible for gathering the information, the information submitted is, to the best of my knowledge and belief, true, accurate, and complete. I am aware that there are significant penalties for submitting false information, including the possibility of fine and imprisonment for knowing violations.

	Name:
	Title:

	Signature:
	Date:





SECTION 12: SWPPP PREPARER CERTIFICATION

	Instructions:
― A SWPPP writer for a site greater than 5 acres, with a perennial surface water within 50 feet of the project, or with a steep slope (70% or 35 degrees or more) must hold a certification to demonstrate that they are a “qualified person” per CGP Part 7. 2.



SWPPP Preparer
I certify under the law that this document and all attachments were prepared under my direction or supervision in accordance with a system designed to assure that qualified personnel properly gathered and evaluated the information submitted. Based on my inquiry of the person or persons who manage the system, or those persons directly responsible for gathering the information, the information submitted is, to the best of my knowledge and belief, true, accurate, and complete. I am aware that there are significant penalties for submitting false information, including the possibility of fine and imprisonment for knowing violations.

	Name:
	Title:

	Signature:
	Date:





SWPPP APPENDICES

Attach the following documentation to the SWPPP: 

Appendix A – Site Maps 
Appendix B – NOI & Authorization to Discharge Letter
Appendix C – UDOT Spill Prevention & Response Plan for Construction Sites
Appendix D – Inspection Reports
Appendix E – Delegation of Authority
Appendix F – Training Logs and Certifications (see CGP 6)
Appendix G – Additional Information (i.e., other permits such as dewatering, stream alteration, wetland; and out of date SWPPP documents)
Appendix I – Construction General Permit


Appendix A: Site Maps

Include any site maps in this appendix. For site map requirements review SWPPP section 7.3.3.



Appendix B: NOI & Authorization to Discharge Letter

Include a copy of your NOI  and the Authorization to Discharge Letter in this appendix. The NOI must be signed.



Appendix C: UDOT Spill Prevention & Response Plan for Construction Sites


Include a copy of UDOT’s Spill Prevention & Response Plan for Construction Sites.
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SPILL PREVENTION and RESPONSE PLAN for  
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The plan contained in the following pages was developed in part from UDOT Construction Division’s  Safety and Health Manual, Section 9 and from the Utah Department of Environmental Quality’s  General Construction Permit, Part 2.3 Pollution Prevention Requirements.

1.0 SPILL PREVENTION AND RESPONSE PLAN 
1.1 General 
This plan is established to provide the Contractor general guidance and procedures to  manage project site operations that have the potential to cause environmental damage when a hazardous spill occurs. The following discharges are prohibited from roadway construction sites and pollution prevention standards are required whenever the sources for these potential pollutants are located on a construction site: 
1. 	Wastewater from washout of concrete; 
2. 	Wastewater from washout and cleanout of paint, form release oils, concrete grinding  slurry, curing compounds, and other construction materials; 
3. 	Fuels, oils, or other pollutants used in vehicle and equipment operation and  maintenance; 
4. 	Soaps, solvents, or detergents used in vehicle and equipment washing; and,
5. 	Toxic or hazardous substances from a spill or other release. 
1.2 Contractor Responsibilities 
The Contractor is responsible for the following requirements: 
1. 	Follow proper procedures for the procurement, receipt, storage, and handling of  hazardous materials under their control. 
2. 	Train employees to control the identified waste and recyclable products in the  containers provided. 
3. 	Maintain Safety Data Sheets (SDS) on file for hazardous chemicals used on  the project and ensure employees follow all of the incorporated requirements. 
4.	Know the potential health and environmental hazards associated with the use of  hazardous materials on the project site. 
5. 	Store and dispose of hazardous or toxic waste in accordance with the manufacturer’s  recommended methods and in compliance with federal, state, tribal, and local  requirements. 
6. 	Inspect hazardous material containments weekly for leaks and damage. 
7. 	Ensure equipment for emergency action is in place to provide quick assistance and  minimize employee risk.
8. 	Use correct personal protective equipment in accordance with the hazard analysis,  SDS, or other procedural requirement. 
1.3 Fueling and Maintenance of Equipment or Vehicles 
If fueling and/or maintenance of equipment or vehicles occur on the project site, the following are required: 
1. 	Ensure adequate supplies are available at all times to handle spills, leaks, and disposal  of used liquids; 
2. 	Use drip pans and absorbents under or around leaky equipment and vehicles; 
3. 	Clean up spills or contaminated surfaces immediately, using dry clean up measures, and eliminate the source of the spill to prevent discharge or a furtherance of an ongoing discharge; and 
4. 	Do not clean surfaces by hosing the area down. 

1.4 Storage of Products that have the Potential to be Hazardous or Toxic Waste 
Examples of hazardous or toxic waste that may be present at construction sites include, but are not limited to, paints, solvents, petroleum‐based products, wood preservatives,  additives, curing compounds, and acids/bases. If storing any of the above products on the construction site, comply with the following: 
1. 	Include the locations of hazardous chemicals and fuels in the SWPPP map.
2. 	Store these products in water‐tight containers away from water flow paths, and provide either cover (e.g., plastic  sheeting or temporary roofs) to prevent these containers from coming into contact with rainwater or provide secondary containment (e.g., spill berms, decks, spill containment pallets)

1.5 Disposal of Waste Products 
1.	For waste disposed of offsite, fill out the UDOT Waste Disposal Tracking Form.   
2.   Separate hazardous or toxic waste from construction and domestic waste. Mixing  increases hazardous waste volume and consequent handling and disposal costs. 
3. 	Store waste in sealed containers, which are constructed of suitable materials to prevent  leakage and corrosion, and which are labeled in accordance with applicable Resource Conservation and Recovery Act (RCRA) requirements and all other applicable state, or local requirements. Provide either cover or secondary containment for waste containers.  
4. 	The Contractor can maintain waste materials and non‐emergency spills up to 2700 lbs.  (approved container) no longer than 180 days from the accumulation start date. Obtain a licensed waste hauler to remove hazardous wastes (liquids, solids). 
5. 	For construction and domestic waste: Provide waste containers (e.g., dumpster or trash receptacle) of sufficient size and number to contain construction and domestic wastes. In addition, clean up and dispose of waste in designated waste containers and clean up immediately if containers overflow. Do not overfill waste containers. If a dumpster is equipped with a drain hole, ensure that it is kept plugged. If a dumpster is equipped with a lid, ensure that it is kept closed and stored away from stormwater conveyance.
6. 	Dispose of hardened concrete waste in ways that are consistent with Utah disposal laws for inert material.
7. 	For sanitary waste: Position portable toilets so that they are secure and will not be tipped or knocked over. Locate portable toilets at least 10 feet away from stormwater conveyances.
1.6 Washout Practices 
Provide an effective means of eliminating the discharge of contaminated water from the washout and cleanout of paint, concrete, form release oils, curing compounds, etc. by incorporating the following: 
1. 	Direct all wash water into a leak‐proof container/pit. The container or pit must be  designed so that no overflows can occur due to inadequate sizing or precipitation.  Segregate paint waste, oily waste, and concrete washout waste and manage the proper disposal separately. 
2.	Ensure liquid wastes are not dumped in storm sewers or surface waters. 
3. 	Locate any washout or cleanout activities as far away as possible from surface waters  and stormwater inlets or conveyances.

1.7 Corrective Actions 
The Contractor must comply with this Hazardous Spill Prevention and Response Plan. The Resident Engineer, the UDOT Environmental Control Supervisor (ECS), and the Region
Stormwater Coordinator (RSC) will monitor the Contractor’s compliance with the plan at the project site. Non‐compliance with spill containment control measures will be communicated to the Contractor by the UDOT RE for immediate corrective action. 

1.8 Spill Control Definition and Control 
1.	Hazardous Spill Definition: A leak, spill, or other release meeting any of the following  measures is a hazardous spill and requires an emergency spill notification (see 1.9.2): 
a. 	2.2 pounds or more of “acutely hazardous waste” (see SDS); or 
b. 	220 pounds or more of other hazardous waste; or, 
c. 	25 gallons or more of fuel or oil are spilled or any amount which causes an oil sheen to form on a water surface. 
2.	Emergency Spill Notification Procedures: If the spill presents a potential for harm to  personnel, public, or the environment, the Contractor is not able to immediately control  and clean‐up the spill, and/or the spill exceeds the reportable quantity (see 1.9.1), the following actions shall be taken: 
a. 	Notify the Resident Engineer and the UDOT ECS to determine if the quantity or severity of the spill warrants outside assistance by emergency services (again, this is to ascertain the toxicity, size of spill, and if the spill could discharge to a surface water or a sewer/storm drain line). The Resident Engineer and UDOT ECS will report the spill to the Region Stormwater Coordinator for further assistance. 
b. 	If the spill is clearly an emergency hazardous spill condition, notify the Utah Department of  Environmental Quality and the National Response Center. 
Emergency Hazardous Spill Notification List 
UDOT Resident Engineer

Utah Department of Environmental Quality  
· 801‐563‐4123 (24-hour emergency line)

National Response Center 
· 800‐424‐8802




c. 	The Contractor is required to use a State Certified Hazardous Materials Lab when necessary to identify an unknown spill material. Identifying the type of spill  material or liquid containment can save the Contractor from increased costs for disposal if the material to be removed is known. 
d. 	The Contractor is responsible for all required hazardous waste management which  includes but is not limited to the transportation, storage, and disposal at a  hazardous waste disposal facility.
3.	Waste Disposal and Minor Spills: A minor spill is a condition that does not present  potential harm to personnel and/or the environment, the Contractor has the ability to  immediately control and clean‐up the spill, and the spill does not meet the hazardous  spill definition. Actions to control non‐emergency spills involve the following activities  from the Contractor: 
a. 	Immediately notify the Resident Engineer for verification that the spill is a non‐ reportable minor spill. 
b. 	Begin spill clean‐up immediately and use trained personnel to respond to critical  events involving spills. 
c.	 Use contingency clean up products and equipment to handle non‐emergency spills  (absorbent materials, personal protection equipment, compatible empty container  to store spilled material, fire extinguisher, etc.) 
d. 	Spilled liquids or solids are to be properly contained in a compatible container and stored onsite until proper disposal action is taken as required by state and federal  requirements. Where a spill occurs or when hazardous wastes are generated, the  Contractor will fill out a hazardous waste label and establish an accumulation date.
e.	If waste was disposed of offsite, fill out the UDOT Waste Disposal Tracking Form: Waste Disposal Tracking Form.    



Appendix D: Inspection Reports

All Contractor and UDOT SWPPP inspections must be completed on UDOT’s approved inspection software at the frequency indicated in Section 8.1.

Include the QR code for the project from ComplianceGo here. 



































Appendix E: Delegation of Authority (CGP 9.9.2)

A delegation of authority form has been included in this appendix. If this is used, keep complete signed forms here.

Delegation of Authority
I, 	, hereby designate the person or specifically described position below to be a duly authorized representative for the purpose of overseeing compliance with environmental requirements, including the UPDES “General Permit for Storm Water Discharges Associated with Construction Activity” (CGP), at the construction site:

	, Permit No. UTR	
The designee is authorized to sign all reports required by the Permit and other information requested by the Director of the Utah Division of Water Quality, or by an authorized representative of the Executive Secretary.

Name of Person or Position: 	

Owner/Operator: 		 Mailing Address: 	
City, State, Zip Code: 		 Phone Number: 	
By signing this authorization, I confirm that I meet the requirements to make such a designation as set forth in Part 9.9.2 of the CGP, and that the designee above meets the definition of a “duly authorized representative” as set forth in Part 9.2.2(b) of the CGP.

I certify under penalty of the law that this document and all attachments were prepared under my direction or supervision in accordance with a system designed to assure that qualified personnel properly gather and evaluate the information submitted. Based on my inquiry of the person or persons who manage the system, or those persons directly responsible for gathering the information, the information submitted is, to the best of my knowledge and belief, true, accurate, and complete. I am aware that there are significant penalties for submitting false information, including the possibility of fine and imprisonment for knowing violations.

Name: 		 Title: 	
Signature: 		 Date: 	




Appendix F: Training Logs and Certifications (see CGP 6)
Environmental Control Supervisor (ECS) Certifications for SWPPP inspectors should be placed in this appendix.

A sample training log has also been included in this appendix to keep track of training that has been provided. At a minimum, stormwater team members that require training should be provided with the following if it relates to their duties (CGP Part 6.3.):
· The permit deadlines associated with installation, maintenance, and removal of stormwater controls and with stabilization;
· The location of all stormwater controls on the site required by this permit and how they are to be maintained;
· The proper procedures to follow with respect to the permit’s pollution prevention requirements; and
· When and how to conduct inspections, record applicable findings, and take corrective actions

Appendix F – Sample SWPPP Training Log
Stormwater Pollution Prevention Training Log

	Project Name:

	Project Location:

	Instructor’s Name(s):

	Instructor’s Title(s):



Course Location: 	 Date: 	 Course Length (hours): 	
Storm Water Training Topic: (check as appropriate)

	❑
	Erosion Control BMPs
	❑
	Emergency Procedures

	❑
	Sediment Control BMPs
	❑
	Good Housekeeping BMPs

	❑
	Non-Storm Water BMPs
	
	



Specific Training Objective:	

Attendee Roster: (attach additional pages as necessary)

	No.
	Name of Attendee
	Company

	1
	
	

	2
	
	

	3
	
	

	4
	
	

	5
	
	

	6
	
	

	7
	
	

	8
	
	

	9
	
	

	10
	
	





Appendix G: Additional Information

Use this appendix for additional information such as other permits (dewatering, stream alteration, etc.) or out of date SWPPP documents.


Appendix I: Construction General Permit

If all storm water team members access the CGP via the internet while on site, the following link to access the Construction General Permit is sufficient:
http://construction.stormwater.utah.gov

Otherwise, include a printed copy of the Construction General Permit in this appendix.
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